Title: Testo di capitolato
Author: RobertoR
Last saved by: Giovanni Schiochet
Company: Giacomini S.p.A.

ekinex® KNX system for
home and building automation

www.ekinex.com
info@ekinex.com

Tender text

ekinex KNX pushbutton Linea71
KNX device for switching and control of single loads or groups of loads and temperature regulation of a single room or zone. Use in home and building automation KNX systems

KNX device for on/off switching of loads, dimmer or blind actuator control. 4 channels with possibility to program up to 8 independent functions. 4 programmable LED for each channel. Integrated temperature sensor and controller for regulation of a single room or zone (control of radiators, radiant panel system, electrical heating). Mounting in round or square flush-mounting box with distance between fixing holes of 60 mm. 

Main functions
•	On/off switching of single loads or groups of loads
•	Dimming of lighting devices
•	Control of motor drives (for roller shutters, blinds, curtains, etc.)
•	Room temperature regulation
•	Sending on the bus of values (temperature, bright-ness, etc.)
•	Switching to forced functioning (lock)
•	Recalling and saving of scenes Measuring of room brightness (not to be used in combination with the set of rockers EK-T1Q-xxx)
•	Different functions programmable for short pressure / long pressure of a rocker
•	Status feedback or orientation nightlight through 2-colour programmable LEDs 

Other characteristics
•	Housing in plastic material
•	Wall installation in flush mounting box 
•	Protection degree IP20 (according to EN 60529)
•	Classification climatic 3K5 and mechanical 3M2 (according to EN 50491-2)
•	Pollution degree 2 (according to IEC 60664-1)   
•	Weight 40 g (70 g with mounting support)
•	Dimensions 81 x 77 x 21 mm (WxHxD) 

Configuration and commissioning
•	Through software ETS4 or later releases
•	Application program for ETS: APEKE13TP##.knxprod (## = release)

Delivery
•	Device
•	Terminal block for connection to the bus line
•	Metallic support for flush-mounting box
•	Fixing screws (2 pairs)

Completion (separate order)
•	set 1 square 60x60 mm rocker or
set 2 rectangular 30x60 mm rockers or
set 4 square 30x30 mm rockers or 4 rectangular 60x15 mm rockers
•	1-fold or 2-fold plate with 60x60 mm window
•	1-fold or 2-fold frame of form or flank series (not for 'NF versions)

Quantity

Order codes: 
EK-E13-TP-BG (mounting with frame, LED colours: blue / green)
EK-E13-TP-RW (mounting with frame, LED colours: red / white)
EK-E13-TP-BG-NF (mounting without frame, LED colours: blue / greeen)
EK-E13-TP-RW-NF (mounting without frame, LED colours: red / white)
Manufacturer: EKINEX S.p.A.

EKINEX S.p.A.
via Novara 37  
28010 Vaprio d’Agogna (NO)

TCEKE13TP_EN.rtf
Rel. 2.0
Updating  10/2022